1. Section 102800   
   Toilet, Bath, and Laundry Accessories - ASI
   1. PART 1  GENERAL
      1. SECTION INCLUDES
         1. Combination units.
      2. RELATED REQUIREMENTS
      3. REFERENCE STANDARDS
      4. SUBMITTALS
         1. See Section 013000 - Administrative Requirements for submittal procedures.
   2. PART 2  PRODUCTS
      1. MANUFACTURERs
         1. Basis of Design Manufacturer:  American Specialties, Inc:  www.americanspecialties.com/#sle.
         2. Other Acceptable Manufacturers:
            1. Products by listed manufacturers are subject to compliance with specified requirements found in specification and in Technical Data Sheet of selected ASI model and prior approval of Architect.
         3. Substitutions:  See Section 016000 - Product Requirements.
            1. All proposed substitutions (clearly delineated as such) must be submitted in writing for approval by Architect minimum of 10 working days prior to bid date and must be made available to all bidders. Proposed substitutes must be accompanied by review of  specification and ASI Technical Data Sheets noting compliance on line-by-line basis.
      2. Combination Units
         1. Combination Toilet Tissue/Seat Cover Dispenser with Napkin Disposal:  Double roll; stainless steel; seamless wall flanges, continuous heavy-duty multi-staked piano hinges, \_\_\_\_.
2. *The paragraph below is optional text*
   * + - 1. Mounting:  As indicated in product listing.
3. *The paragraph below is optional text*
   * + - 1. Door:  Seamless 18 gauge, 0.05 inch (1.3 mm) door with returned edges and tumbler lock.
4. *The paragraph below is optional text*
   * + - 1. Cabinet:  Fully welded, 22 gauge, 0.03 inch (0.8 mm) thick stainless steel.
5. *The paragraph below is optional text*
   * + - 1. Minimum Capacity:  1,000 seat covers.
6. *The paragraph below is optional text*
   * + - 1. Waste Receptacle Capacity:  1.3 gal (4.9 L).
         2. Products:

Model 0487-L-9 - Surface Mounted - Traditional Collection - Toilet Seat Cover and Toilet Tissue Dispenser with Sanitary Napkin Disposal - Horizontal, ADA.

1. *The paragraph below is optional text*

Substitutions:  Section 016000 - Product Requirements.

* + 1. Fabrication
       1. Traditional Collection:
          1. Basic Construction Requirements:

Doors:  Type 304, 22 gauge, 0.0312 inch (0.79 mm) stainless steel, double pan construction, with 1/4 inch (6 mm) thick structural fiberboard core.

Cabinets:  Type 304, 22 gauge, 0.0312 inch (0.79 mm) stainless steel, formed perimeter trim with 1/4 inch (6 mm) return to wall four sides; joints welded, sight-exposed welds finished to match sheet finish.

Hinges:  Heavy-duty stainless steel multi-staked piano hinge, 3/16 inch (5 mm) diameter barrel, full length of cabinet; hinge leaves spot-welded to door and cabinet body.

Locks:  Tumbler locks, keyed alike other toilet accessory locks, with one key for each lock.

Cabinet and Door Finish:  No.4 satin finish.

* 1. PART 3  EXECUTION
     1. EXAMINATION
        1. Verify existing conditions before starting work.
        2. Verify exact location of accessories for installation.
     2. PREPARATION
        1. Deliver inserts and rough-in frames to site for timely installation.
        2. Provide templates and rough-in measurements as required.
     3. INSTALLATION
        1. Install accessories in accordance with manufacturers' instructions in locations indicated on drawings.
        2. Mounting Heights:  As required by accessibility regulations, unless otherwise indicated.
           1. Other Accessories:  As indicated on drawings.
     4. PROTECTION
        1. Protect installed accessories from damage due to subsequent construction operations.

1. END OF SECTION